%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

%CFD Project 4

%Program 1

%Transient advection diffusion equation

%Central difference second order in space

%AB2 in time

%

%Author: Jithin Gopinadhan

%Date : 11/30/2015

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

clc

clear all

L=2\*pi(); %Length of domain

N=[20 40 80 160]; %Grid sizes

Time=10; %Maximum time for simulation

dt=0.0001; %Delta t

M=Time/dt; %Number of iterations in time

%Initializing error matrices for different grid sizes

Err20=zeros(N(1)-1);

Err40=zeros(N(2)-1);

Err80=zeros(N(3)-1);

%Initializing matrix to save data at x=3pi/4 and y=pi/4

Pos\_data\_x=zeros(5,N(4)+1);

Pos\_data\_y=zeros(5,N(4)+1);

%This loop runs for the different grid

%sizes specified above

for grid=1:4

h=L/N(grid); %Symmetric grid: delta x = delta y = h

%Initializing temperature and its time derivative

%for two steps in time

Tn=zeros(N(grid)+1); %Temperature at nth time

Tnp1=zeros(N(grid)+1); %Temperature at (n+1)th time

dTn=zeros(N(grid)+1); %dT/dt value at current time step

dTnm1=zeros(N(grid)+1); %dT/dt value at previous time step

%Initializing boundary conditions

for i=1:N(grid)+1

Tn(1,i)=1;

Tn(N(grid)+1,i)=1;

end

%Time loop

for t=0:dt:Time

%Spatial loops

for i=1:N(grid)+1

for j=1:N(grid)+1

x=h\*(i-1);

y=h\*(j-1);

u=sin(x)\*cos(y); %Velocity components

v=-cos(x)\*sin(y);

%Interior points

if(i>1 && i<(N(grid)+1) && j>1 && j<(N(grid)+1))

%Evaluation of individual terms

dTx= (Tn(i+1,j)-Tn(i-1,j))/(2\*h);

dTy= (Tn(i,j+1)-Tn(i,j-1))/(2\*h);

d2Tx= (Tn(i+1,j)- 2\*Tn(i,j)+Tn(i-1,j))/(h^2);

d2Ty= (Tn(i,j+1)- 2\*Tn(i,j)+Tn(i,j-1))/(h^2);

%Evaluation of dT/dt

dTn(i,j) = -u\*dTx - v\*dTy + d2Tx + d2Ty;

end

end

end %End of spatial loops

%Using first order for t=0

if(t==0)

Tnp1 = Tn + (dTn \*dt);

end

%Using AB2 for all other

if(t>0)

Tnp1 = Tn + (0.5\*dt)\*(3\* dTn - dTnm1);

end

%Assigning T and dT/dt values to correct variable

%before stepping forward in time

Tn=Tnp1;

dTnm1=dTn;

%Plotting temperature profile for required times

if(t==2.5 || t==5 || t==7.5 || t==10)

[X,Y] = meshgrid(0:h:2\*pi());

figure,mesh(X,Y,Tnp1)

s1=num2str(t);

s2=num2str(N(grid));

title(['Temperature distribution at t=',s1,'(',s2,'x',s2,')'] ,'FontSize',10)

xlabel('y');

ylabel('x');

end

%Evaluation of T along x=3\*pi/4 and y=pi/4

%for required times at highest grid resolution

if(grid==4 && (t==2.5 || t==5 || t==7.5 || t==10))

T80=Tn;

i\_pos=(3\*N(grid) +8)/8; %3pi/4

j\_pos=(N(grid) +8)/8; %pi/4

x\_pos=3\*pi()/4;

y\_pos=pi()/4;

%Finding index of next highest nodes

i\_ceil=ceil(i\_pos);

j\_ceil=ceil((j\_pos));

%Finding position of adjacent nodes

x1= (i\_ceil-2)\*h;

x2= (i\_ceil-1)\*h;

y1= (j\_ceil-2)\*h;

y2= (j\_ceil-1)\*h;

for q=1:N(grid)+1

%Linear interpolation of temperature based on temperature

%values of adjacent nodes

T\_xpos=T80(i\_ceil-1,q)+ (T80(i\_ceil+1,q)-T80(i\_ceil-1,q))\*((x\_pos-x1)/h);

T\_ypos=T80(q,j\_ceil-1)+ (T80(q,j\_ceil+1)-T80(q,j\_ceil-1))\*((y\_pos-y1)/h);

len=(q-1)\*h;

%Saving data for plotting later

Pos\_data\_x(q,1)=len;

Pos\_data\_x(q,(t/2.5)+1)=T\_xpos;

Pos\_data\_y(q,1)=len;

Pos\_data\_y(q,(t/2.5)+1)=T\_ypos;

end

end

end %End of time loop

%Saving values at t=10 for grid refinement study

if(grid==1)

T20=Tn;

end

if(grid==2)

T40=Tn;

end

if(grid==3)

T80=Tn;

end

if(grid==4)

T160=Tn;

end

end

%Evaluation of errors of 3 lower grid refinements against

%highest grid refinemnt assuming it to be exact

for i=1:N(1)-1

for j=1:N(1)-1

Err20(i,j)=T160((1+i\*8),(1+j\*8))-T20(i+1,j+1);

end

end

for i=1:N(2)-1

for j=1:N(2)-1

Err40(i,j)=T160((1+i\*4),(1+j\*4))-T40(i+1,j+1);

end

end

for i=1:N(3)-1

for j=1:N(3)-1

Err80(i,j)=T160((1+i\*2),(1+j\*2))-T80(i+1,j+1);

end

end

%Evaluation of L2 norm for errors

E20=norm(Err20)/(N(1)-1); E40=norm(Err40)/(N(2)-1); E80=norm(Err80)/(N(3)-1);

%Evaluation of order of convergence

order=log((E80-E40)/(E40-E20))/log(0.5)

%Plotting temperature profiles along x=3pi/4

figure,plot(Pos\_data\_x(:,1),Pos\_data\_x(:,2),'.-')

hold on

plot(Pos\_data\_x(:,1),Pos\_data\_x(:,3),'.-')

hold on

plot(Pos\_data\_x(:,1),Pos\_data\_x(:,4),'.-')

hold on

plot(Pos\_data\_x(:,1),Pos\_data\_x(:,5),'.-')

title('Temperature at x= 3pi/4','FontSize',12)

xlabel('y');

ylabel('Temperature');

legend('t=2.5','t=5','t=7.5','t=10')

%Plotting temperature profiles along y=pi/4

figure,plot(Pos\_data\_y(:,1),Pos\_data\_y(:,2),'.-')

hold on

plot(Pos\_data\_y(:,1),Pos\_data\_y(:,3),'.-')

hold on

plot(Pos\_data\_y(:,1),Pos\_data\_y(:,4),'.-')

hold on

plot(Pos\_data\_y(:,1),Pos\_data\_y(:,5),'.-')

title('Temperature at y= pi/4','FontSize',12)

xlabel('x');

ylabel('Temperature');

legend('t=2.5','t=5','t=7.5','t=10')